[PhoneCommonInfo]
Version=1.0
Comments=Driver for Siemens X65
Copyright=Chaos, Ported to V_Klay by ValeraVi
ReleaseDate=2004-12-06
Name=CX65/M65/S65
MCUMemGeometry=0
optBaudCmdCodes=57600: 0x00, 115200: 0x01, 230400: 0x02, 460800: 0x03, 614400: 0x04, 921600: 0x05, 1228800: 0x06, 1600000: 0x07,
optCmdAddrAndSizeLen=4
optWriteCmdVersion=2
optTestEmptyCmdEnable=1
optKeepAliveCmdEnableAndSetInterval=250
Boots=Connect, GoBoot.bin, MainBoot.bin, ChaosKey1.bin, ChaosKey2.bin
Type=Password boot

[Phone01]
Name=C65 354736009926644
Comments=Siemens C65 Phone (connecting, using boot password)
MCUMemFuBu=   fullflash,        0xA0000000, 0x02000000
MCUMemArea01= bootcore,         0xA0000000, 0x00020000, bootcore
MCUMemArea02= EEFULL,           0xA0220000, 0x00040000
MCUMemArea05= EELITE,           0xA0FE0000, 0x00020000


[Boot01]
Name=Connect
UseIgnition=1
TryCount=-1
NoSendLen=1
Data=0sAT
NoSendCheckSum=1
Answer=B0
AnswerTimeout=100

[Boot02]
Name=GoBoot.bin
NoSendLen=1
Data=30
NoSendCheckSum=1

[Boot03]
Name=MainBoot.bin
SizeLen=2
[encoded data, 5261 characters]
Answer=B1

[Boot04]
Name=ChaosKey1.bin
DelayBefore=100
NoSendLen=1
Data=E236E44A03DC
NoSendCheckSum=1

[Boot05]
Name=ChaosKey2.bin
DelayBefore=100
NoSendLen=1
Data=91331F7E9AB181CF6DBB261C9C3A3F2C9F29FF9AECF1EA96501D76CF753A4416341A75DA990112B62EE4F6C880
NoSendCheckSum=1
Answer=A5

