[PhoneCommonInfo]
Version=1.0
Comments=Driver for Siemens X75
Copyright=Chaos, Ported to V_Klay by ValeraVi
Name=R65/X75
MCUMemGeometry=0
optBaudCmdCodes=57600: 0x00, 115200: 0x01, 230400: 0x02, 460800: 0x03, 614400: 0x04, 921600: 0x05, 1228800: 0x06, 1600000: 0x07,
optCmdAddrAndSizeLen=4
optWriteCmdVersion=2
optTestEmptyCmdEnable=1
optKeepAliveCmdEnableAndSetInterval=250
[Phone01]
Name=S75
Boots=ConnectX75, GoBoot.bin, BootX75.bin, Test.bin
Type=BootKey, Skey and NewFlash
Comments=Siemens  Phone S/SL75 (connecting, using boot password)
MCUMemFuBu= fullflash, 0xA0000000, 0x04000000
MCUMemArea01= BCORE,   0xA0000000, 0x00020000, bootcore
MCUMemArea02= EELITE,  0xA0040000, 0x00020000
MCUMemArea03= CODE,    0xA0080000, 0x0140A000
MCUMemArea04= LngPack, 0xA1640000, 0x002D0000
MCUMemArea05= GFXPack, 0xA19A0000, 0x00220000
MCUMemArea06= FFS_A,   0xA1C00000, 0x01BC0000
MCUMemArea07= FFS_C,   0xA37C0000, 0x00200000
MCUMemArea08= FFS_B,   0xA39C0000, 0x005E0000
MCUMemArea09= EEFULL,  0xA3FA0000, 0x00040000
MCUMemArea10= SEXIT,   0xA3FE0000, 0x00020000
[Phone02]
Name=S65
Boots=ConnectR65, GoBoot.bin, BootR65.bin, Test.bin
Type=BootKey, Skey and NewFlash
Comments=Siemens R65 Phone (connecting, using boot password or new/clear flash)
MCUMemFuBu= fullflash, 0xA0000000, 0x02000000
MCUMemArea01= BCORE,  0xA0000000, 0x00020000, bootcore
MCUMemArea02= CODE1,  0xA0020000, 0x001E0000
MCUMemArea03= EXIT,   0xA0200000, 0x00020000
MCUMemArea04= EEFULL, 0xA0220000, 0x00040000
MCUMemArea05= FFS_B,  0xA0260000, 0x00080000
MCUMemArea06= FFS_C,  0xA02E0000, 0x00200000
MCUMemArea07= FFS_A1, 0xA04E0000, 0x00320000
MCUMemArea08= XCORE,  0xA0800000, 0x00020000
MCUMemArea09= CODE2,  0xA0820000, 0x007C0000
MCUMemArea10= EELITE, 0xA0FE0000, 0x00020000
MCUMemArea11= CODE3,  0xA1000000, 0x00800000
MCUMemArea12= FFS_A2, 0xA1800000, 0x00800000
[Boot01]
Name=ConnectX75
UseIgnition=1
TryCount=-1
NoSendLen=1
Data=0sAT
NoSendCheckSum=1
Answer=C0
AnswerTimeout=20
[Boot03]
Name=GoBoot.bin
NoSendLen=1
Data=30
NoSendCheckSum=1
[Boot02]
Name=BootX75.bin
SizeLen=2
Data01=120000EA0000000000000000000000000000000000000000000000000000000000000000000000005349454D454E535F424F4F54434F44450300000000000000
Data02=970DE2E0BEC452CEB1F5B3D2D9724A3B
[encoded data, 4327 characters]
Answer=C1A5
[Boot04]
Name=Test.bin
DelayBefore=200
NoSendLen=1
Data=41
NoSendCheckSum=1
Answer=52
[Boot05]
Name=ConnectR65
UseIgnition=1
TryCount=-1
NoSendLen=1
Data=0sAT
NoSendCheckSum=1
Answer=B0
AnswerTimeout=20
[Boot06]
Name=BootR65.bin
SizeLen=2
Data01=120000EA0000000000000000000000000000000000000000000000000000000000000000000000005349454D454E535F424F4F54434F44450300000000000000
Data02=970DE2E0BEC452CEB1F5B3D2D9724A3B
[encoded data, 4327 characters]
Answer=B1A5
