[PhoneCommonInfo]
Version=1.0
Comments=Driver for Siemens x65
Copyright=Chaos, Ported to V_Klay by ValeraVi
ReleaseDate=2006-02-21
Name=Siemens x65
MCUMemGeometry=0
optBaudCmdCodes=57600: 0x00, 115200: 0x01, 230400: 0x02, 460800: 0x03, 614400: 0x04, 921600: 0x05, 1228800: 0x06, 1600000: 0x07,
optCmdAddrAndSizeLen=4
optWriteCmdVersion=2
optTestEmptyCmdEnable=1
optKeepAliveCmdEnableAndSetInterval=250
Boots=Connect, GoBoot.bin, Boot.bin, Test.bin
Type=Password Boot

[Phone01]
Name=357985006668728
Comments=Siemens x65 Phone (connecting, using boot password)
MCUMemFuBu=   fullflash,        0xA0000000, 0x02000000
MCUMemArea01= bootcore,         0xA0000000, 0x00020000, bootcore
MCUMemArea02= EEFULL,           0xA0220000, 0x00040000
MCUMemArea05= EELITE,           0xA0FE0000, 0x00020000


[Boot01]
Name=Connect
UseIgnition=1
TryCount=-1
NoSendLen=1
Data=0sAT
NoSendCheckSum=1
Answer=B0
AnswerTimeout=20

[Boot02]
Name=GoBoot.bin
NoSendLen=1
Data=30
NoSendCheckSum=1

[Boot03]
Name=Boot.bin
SizeLen=2
[encoded data, 4589 characters]
Answer=B1A5

[Boot04]
Name=Test.bin
DelayBefore=200
NoSendLen=1
Data=41
NoSendCheckSum=1
Answer=52

